Moisture content process TEMPLATE

*This is a template. Please align the template to your own process.*

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Time | Reference | Moisture content |
|  |  |  |  |

Recommended process:

We recommend taking at least 3 logs from your dry pile/stack to test. Split the log down the center ensuring you measure the moisture content from the newly exposed center of the log, pressing the meter pins across the grain. Record 3 measurements, 2 from the top, 2 from the middle, 2 from the bottom. Record this and use the average moisture content for that log.

Your process:

* We follow Woodsure’s recommended moisture content check process
* We follow the below moisture content check process (please outline this in the below and answer the following questions)
1. How often are you moisture checking your log pile?.................................
2. How is the firewood tested?......................................................................
3. What do you use to take the moisture reading?........................................
4. How is the fuel packaged?.........................................................................
5. What is your process if the wood is testing over 20%?.............................

|  |
| --- |
| *Pictures of your process are encouraged.* |

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Time | Reference | Moisture content |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |